
No smart combiners? No problem.

Monitor the DC side of your system for subcombiner and recombiner data.



## Features

* NEMA 4 rated enclosure
* Plug and play installation
* 5 year warranty
* 10 channel iputs for up to 10 zones
* Split-Core DC CTs for easy installation and replacements
* No need to route DC feeders through the enclosure, CT leads extend up to 30’
* CTs avaiale for 250 A and greater

|  |  |  |  |
| --- | --- | --- | --- |
|  | |  | |
| Part ID | Veris EA20BB020 |  |  |
|  | 0-200A |  |  |
|  | 4-20mA Output |  |  |
| Window | 1 1/8” |  |  |
|  |  |  |  |
|  | |  |  |
| Part ID | CTH-401LST |  |  |
|  | 0-400A |  |  |
|  | 4-20mA ouput |  |  |
| Window | 1 1/8” |  |  |
|  |  |  |  |
| Higher Amperage models avaiable | |  |  |